# Static Call Graph for image .\Objects\VGA.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Mon Feb 02 15:24:19 2015

### Maximum Stack Usage = 40 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ VGA_beallitasa ⇒ kep_kimenet_beallitasa ⇒ GPIO_Init

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from vga.o(i.DMA1_Channel1_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SysTick_Handler from systick_kesleltetes.o(i.SysTick_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from vga.o(i.TIM2_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from vga.o(i.TIM3_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_md.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  DMA1_Channel1_IRQHandler (Thumb, 72 bytes, Stack size 0 bytes, vga.o(i.DMA1_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_DeInit))
  [Called By]

  - >> DMA_beallitasa

  DMA_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_ITConfig))
  [Called By]

  - >> DMA_beallitasa

  DMA_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_dma.o(i.DMA_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> DMA_beallitasa

  DMA_beallitasa (Thumb, 104 bytes, Stack size 8 bytes, vga.o(i.DMA_beallitasa))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA_beallitasa ⇒ NVIC_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> NVIC_Init
  - >> DMA_Init
  - >> DMA_ITConfig
  - >> DMA_DeInit
  [Called By]
  - >> VGA_beallitasa

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> kep_kimenet_beallitasa
  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> TIM3_beallitasa
  - >> TIM2_beallitasa
  - >> DMA_beallitasa

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_AHBPeriphClockCmd))
  [Called By]

  - >> DMA_beallitasa

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> kep_kimenet_beallitasa
  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  SysTick_Handler (Thumb, 18 bytes, Stack size 0 bytes, systick_kesleltetes.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SysTick_Inditasa (Thumb, 84 bytes, Stack size 8 bytes, systick_kesleltetes.o(i.SysTick_Inditasa))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Inditasa
  [Called By]
  - >> main

  SysTick_Kesleltetes_ms (Thumb, 62 bytes, Stack size 0 bytes, systick_kesleltetes.o(i.SysTick_Kesleltetes_ms))
  [Called By]

  - >> main

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  TIM2_IRQHandler (Thumb, 112 bytes, Stack size 0 bytes, vga.o(i.TIM2_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM2_beallitasa (Thumb, 160 bytes, Stack size 8 bytes, vga.o(i.TIM2_beallitasa))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM2_beallitasa ⇒ GPIO_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_SelectOutputTrigger
  - >> TIM_SelectMasterSlaveMode
  - >> TIM_OC1Init
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> GPIO_Init
  [Called By]
  - >> VGA_beallitasa

  TIM3_IRQHandler (Thumb, 78 bytes, Stack size 0 bytes, vga.o(i.TIM3_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_beallitasa (Thumb, 158 bytes, Stack size 8 bytes, vga.o(i.TIM3_beallitasa))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM3_beallitasa ⇒ GPIO_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_SelectSlaveMode
  - >> TIM_SelectInputTrigger
  - >> TIM_OC1Init
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> GPIO_Init
  [Called By]
  - >> VGA_beallitasa

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_Cmd))
  [Called By]

  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ITConfig))
  [Called By]

  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  TIM_OC1Init (Thumb, 132 bytes, Stack size 16 bytes, stm32f10x_tim.o(i.TIM_OC1Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_OC1Init
  [Called By]
  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_SelectInputTrigger))
  [Called By]

  - >> TIM3_beallitasa

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_SelectMasterSlaveMode))
  [Called By]

  - >> TIM2_beallitasa

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_SelectOutputTrigger))
  [Called By]

  - >> TIM2_beallitasa

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_SelectSlaveMode))
  [Called By]

  - >> TIM3_beallitasa

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_TimeBaseInit))
  [Called By]

  - >> TIM3_beallitasa
  - >> TIM2_beallitasa

  VGA_beallitasa (Thumb, 24 bytes, Stack size 8 bytes, vga.o(i.VGA_beallitasa))
  [Stack]

  - Max Depth = 40
  - Call Chain = VGA_beallitasa ⇒ kep_kimenet_beallitasa ⇒ GPIO_Init
  [Calls]
  - >> kep_kimenet_beallitasa
  - >> VGA_kepernyo_torles
  - >> TIM3_beallitasa
  - >> TIM2_beallitasa
  - >> DMA_beallitasa
  [Called By]
  - >> main

  VGA_kepernyo_torles (Thumb, 76 bytes, Stack size 0 bytes, vga.o(i.VGA_kepernyo_torles))
  [Called By]

  - >> VGA_beallitasa

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  kep_kimenet_beallitasa (Thumb, 32 bytes, Stack size 8 bytes, vga.o(i.kep_kimenet_beallitasa))
  [Stack]

  - Max Depth = 32
  - Call Chain = kep_kimenet_beallitasa ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> VGA_beallitasa

  main (Thumb, 100 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 40
  - Call Chain = main ⇒ VGA_beallitasa ⇒ kep_kimenet_beallitasa ⇒ GPIO_Init
  [Calls]
  - >> VGA_beallitasa
  - >> SysTick_Kesleltetes_ms
  - >> SysTick_Inditasa
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  ### Undefined Global Symbols