# **PIC 18F USB to Serial & MPLAB Code Configurator**

This demonstrates the how install the MPLAB Code Configurator on the MPLAB X IDE and using it to generate code for USB to Serial device on a PIC microcontroller. Using the XC8 compiler with MPLAB X and a PIC18F45k50.

[![PIC Programming Tutorial #28 - USB to Serial & MPLAB Code Configurator](https://img.youtube.com/vi/GXDTH1TGD1w/0.jpg)](https://www.youtube.com/watch?v=GXDTH1TGD1w "PIC Programming Tutorial #28 - USB to Serial & MPLAB Code Configurator")

☕Coffee Funds☕.

Shekels: 
https://www.paypal.me/bindertronics9/5

Patreon:
https://www.patreon.com/BinderTronics

Bitcoin: 
19nohZzWXxVuZ9tZvw8Pvhajt5khG5mspW

Ethereum: 
0x5fe29789CDaE8c73C9791bEe36c7ad5db8511D39
