MJoy schematic version 1.4 Parts List

| Component | Value | Quanitity | Designator | Remarks |
| Microcontroller | ATMEGA8-16PI | 1 | U1 |  |
| Crystal Oscilator | 12MHz | 1 | Q1 |  |
| Zener diode | 1N4733 | 2 | D1, D2 | May be any 3.3V zener diode. |
| Diode | 1N4148 | 28 | D3-D30 | May be any low power silicon diode. |
| Resistor | 2.2k | 1 | R1 |  |
| Resistor | 4.7k | 1 | R2 |  |
| Resistor | 82 Ohm | 2 | R3, R4 |  |
| Resistor | 330 Ohm | 4 | R5-R8 |  |
| Potentiometer | 10k | 6 | R9-R14 | 10k is recommended but potentiometer of any greater value up to 100k may be used. |
| Capacitor | 10uF | 1 | C1 | Polar capacitor. |
| Capacitor | 15pF | 2 | C2, C3 |  |
| Capacitor | 0.1uF | 3 | C4-C6 |  |
| Inductor | 10uH | 1 | L1 | Or some similar value. Can use a simple wire instead if inductor is not available. |
| Socket | USB type B | 1 | J1 | May be omitted if USB cable is soldered directly into PCB. |
| Connector | DB-25 male | 1 | J2 |  |
| Socket+Connector | 5-pin | 1 | JP1, JP2 | Or some other pair with more than 5 pins. |
| Socket+Connector | 3-pin | 6 | JP3-JP8 | Or some other pair with more than 3 pins. |
| Socket+Connector | 11-pin | 1 | - | If buttons are connected to PCB through socket any 11 or more pin socket/connector pair may be used. |
| Button | Pushbutton | 24 | S1-S24 |  |
| Hatswitch | Hatswitch | 1 | UP-LEFT |  |