AT  
OK  
ATR0    
OK  
ATO1    
OK  
ATF?    
OK  

Inquiry Results:                
1  pagabee           6C0E-0D-BE1062                                   
2  USER-6A356E5D5C   0027-13-A27392                                   
AT  
 already stoped searching!                          

OK  
ATD=6C0E0DBE1062                
OK  
ATA   
OK  

CONNECT  '6C0E-0D-BE1062'                         
AT  
OK  
ATI				  a GSM modem válasza
Sony Ericsson J105

OK
+++
OK
ATI1
OK
ATC=1, HARDWARE FLOW CONTROL
ATD=6C0E-0D-BE1062, SET BLUETOOTH ADDRESS CONNECT TO
ATE=1, ECHO CHARACTERS
ATG=1, ENABLE ALL PAGE AND INQUIRY SCAN
ATH=1, DISCOVERABLE
ATK=0, ONE STOP BIT
ATL=5, BAUD RATE is 115200
ATM=0, NONE PARITY_BIT
ATN=BTM112 Module, LOCAL NAME
ATO=1, DISABLE AUTO CONNECTING
ATP=1357, PIN CODE
ATQ=0, SEND RESULT CODE
ATR=0, SPP MASTER ROLE
ATS=1, ENABLE AUTO-POWERDOWN OF RS232 DRIVER
ATX=1, ALWAYS CHECK '+++'
