
Assalam O Alaikum.


This Simulink model has been posted in collaboration with Alex Rodriguez who
orignally uploaded it, however as you would have know his file does not run,
I have removed the errors from it and now it can simulate the data rate of 12.2 Kbps.

There are still some problems with the model for higer data rates. When I get 
time I'll debug that also. However, I upload the model for those who need it and
might be able to debug the errors themselves. I shall be there to help you
if needed. Please let me know if you are able to improve the model.

Your will need to understand 3GPP standards 25.211 v3.6.0, 25.212 v3.6.0, 
25.101 v3.6.0,and 25.213 v3.6.0 from www.3gpp.org

The Simulator simulates the Physical layer of UMTS Rel 99 for downlink.

Please be advised that you must first open wcdmademos.mdl>wcdmaPhysicallayer.mdl
and then open my WCDMAPhysicallayer3.mdl, as you wont have the WCDMA blocks in 
your library


Contact me:

Syed Mohammed Zafi Sherhan Shah

Bachelors in Telecommunications Engineering,
Mehran University of Engineering & Technology,
Jamshoro, Sindh. Pakistan

<shah_zafi@yahoo.com>